{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":238,"n_cols":9,"rows_kept":238,"cut":false,"hidden":false,"merged":[[2,0,2,8],[3,4,3,7],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,8,4,8],[0,0,1,8]]}
["仪器设备一览表"]
[]
[]
["序号","仪器设备名称","规格型号","出厂编号","技术指标",null,null,null,"制造厂家/供应商"]
[{"$nulls":4},"量程","准确度/等级","测量不确定度","分辨率"]
[1,"建筑门窗隔声性能检测装置","GS-Ⅰ","20-012","100Hz~5000Hz",null,null,"1Hz","沈阳合兴检测设备有限公司"]
[2,"建筑门窗三性检测仪","XMCY-2424","21-021","水流计：0~1600L/h\n风压变送器：-600~600Pa，-7000~7000Pa\n位移计：0~50mm",null,null,"/","沈阳合兴检测设备有限公司"]
[3,"建筑外门窗保温性能检测装置","BWC-II","21-043","-30~30℃",null,null,"0.1℃","沈阳合兴检测设备有限公司"]
[4,"建筑幕墙物理性能检测设备","MW-K80120B","20-07","气流量：0~3500m3/h\n风压值：-10000~12000Pa\n喷淋量：250~25000L/h",null,null,"/","沈阳紫微恒检测设备有限公司"]
[5,"隔热型材传热系数测定装置","BHR2424","2021-023",{"$nulls":4},"北京中科天昊科技有限公司"]
[6,"耐火完整性实验装置","TH-NHL-1","2021-101",{"$nulls":4},"北京中科天昊科技有限公司"]
[7,"燃烧环保除尘设备","定制"]
[8,"门窗抗风携碎物试验机","MCSC-1515","2021-132",{"$nulls":4},"北京中科天昊科技有限公司"]
[9,"大理石平台","1500×2000mm"]
[10,"电子引伸计","YYU-25/25",213164,"25mm","1级",null,null,"钢研纳克检测技术股份有限公司"]
[11,"水平尺","GWP-91B 1000mm",null,"1000mm",null,null,null,"长城精工"]
[12,"微机控制电子万能试验机","WDW-50","072","50kN","1级",null,"1N","济南天辰试验机制造有限公司"]
[13,"高低温材料试验箱","GR7080",201405003,"-40～120℃",null,null,"1℃","济南天辰试验机制造有限公司"]
[14,"高低温试验箱","GDW-50A",202108005,"-30～100℃",null,null,"1℃","济南天辰试验机制造有限公司"]
[15,"微机控制电子万能试验机","WDW-20G","064","20KN","0.5级",null,"0.1N","济南天辰试验机制造有限公司"]
[16,"轴向引伸计","E108560","3542-050M-050-ST","50mm",null,null,null,"Epsilon technology corp"]
[17,"微机控制电子万能试验机","WDW-10G","075","10KN","0.5级",null,"0.1N","济南天辰试验机制造有限公司"]
[18,"IP65数显千分尺","0-25mm G103","C27667","25mm",null,null,"0.001mm","上海量具刃具厂有限公司"]
[19,"引伸计","BT2-EXMACRO.ETH.H11",260553]
[20,"电子万能材料试验机","Z100",736171,"10t/1t","1级",null,"0.1N","Zwick/Roell"]
[21,"应力腐蚀试验机","CFS-50","210A001","50kN\n80mm\n350℃",null,null,"0.3N\n0.1μm\n1℃","上海凯尔孚应力腐蚀试验设备有限公司"]
[22,"高温持久荷载试验箱","GCF-10010","01","100℃",null,null,null,"济南天辰试验机制造有限公司"]
[23,"动静万能试验系统","PWS-50",370,"50KN\n振幅75mm\n0.01-50HZ",null,null,null,"济南东侧试验机技术有限公司"]
[24,"高低温试验箱","GDW-80",10910,"-40～200℃",null,"±0.5℃",null,"济南东侧试验机技术有限公司"]
[25,"机器人操控耐久性测试系统","SARTS-NWT-A","20-02",{"$nulls":4},"沈阳紫薇恒检测设备有限公司"]
[26,"温湿度表","GJWS-小A2",null,"0-40℃、0-90%RH",null,null,"1℃、2%RH"]
[27,"电子数显百分表","0-25.4mm","DN191271","25.4mm",null,null,"0.001mm"]
[28,"电子数显百分表",{"$nulls":5},"0.001mm"]
[29,"数显扭矩扳子","YHSX-50",400766009,"50Nm",null,null,null,"四川远跃恒电子"]
[30,"数显扭矩扳子","YHSX-4",400766007,"4Nm",null,null,null,"四川远跃恒电子"]
[31,"指针式推拉力计","NK-500","081026222",{"$nulls":4},"乐清市麦克斯测控设备厂"]
[32,"数显式推拉力计","HP-100","H1002003983"]
[33,"数显式推拉力计","HP-200","H2002007968"]
[34,"建筑外窗采光性能检测装置","JZCG","21-008","200000lux",null,null,null,"沈阳合兴检测设备有限公司"]
[35,"慢走丝线切割机床","SPWQ400","A4356",{"$nulls":4},"Sodick（Thailand）Co.，Ltd."]
[36,"加工中心","VMC855",2110068,{"$nulls":4},"山东鲁南机床设备有限公司"]
[37,"数控车床","CLK6140D/1",2021119,{"$nulls":4},"山东鲁南机床设备有限公司"]
[38,"锯铝机"]
[39,"铣钻床","ZX7032",1103001,{"$nulls":4},"杭州西湖台钻有限公司"]
[40,"电火花高速小孔加工机","DD703",211131,{"$nulls":4},"苏州雅玛格数控装备有限公司"]
[41,"台式砂轮机","MD3220 200mm",{"$nulls":5},"常熟市古理特电机厂泽国分厂"]
[42,"数显千分尺","IP65 0-25mm","293-240-30",null,null,null,"0.001mm","Mitutoyo"]
[43,"台虎钳"]
[44,"电阻炉"]
[45,"手提式高压蒸汽灭菌器","DSX-18L-1","21G210178","0.142MPa、126℃",null,null,null,"上海申安医疗器械厂"]
[46,"数显恒温磁力搅拌器","1995-02-01",{"$nulls":5},"常州荣华仪器制造有限公司"]
[47,"酸碱滴定管"]
[48,"实验室级超纯水机","SMART-S2-10DS",2107192701,{"$nulls":4},"南京易普易达科技发展有限公司"]
[49,"分光色彩精灵 45/0光泽",6801,"680100001340205",{"$nulls":4},"毕克化学（铜陵）有限公司"]
[50,"数字涡流金属电导仪","sigma2008",8001519,null,null,null,"0.1MS/m","厦门天研仪器有限公司"]
[51,"QFH型漆膜划格器","QFH型",210618,"1、2、3mm",null,null,null,"天津建科试验仪器厂"]
[52,"电热恒温水浴锅","SYG-2-4",2303317,"室温+5～100℃",null,"±0.5℃",null,"天津市泰斯特仪器有限公司"]
[53,"表面粗糙度仪","TR200",16030814,{"$nulls":4},"时代集团公司"]
[54,"自动划痕仪","ZHY",{"$nulls":5},"上海普申化工机械有限公司"]
[55,"便携式铅笔划痕试验仪","QHQ-A型",{"$nulls":5},"天津永利达材料试验机有限公司"]
[56,"巴克霍尔兹压痕试验仪","QHY",{"$nulls":5},"天津永利达材料试验机有限公司"]
[57,"氙灯老化试验机","Q-SUN XE-3-HS","20-17001-77-X3HS",{"$nulls":4},"Q-Lab Corporation"]
[58,"摩尔纯水机","MOLFOG10A","2020-3-94",{"$nulls":4},"重庆摩尔水处理设备有限公司"]
[59,"臭氧老化试验箱","QL-100C",202108145,"20-65℃、30-98%RH、20-500PPHM",null,"±2℃",null,"南京环科试验设备有限公司"]
[60,"中空玻璃高低温交变湿热试验箱","HW/SQMF-010B",20230104001,"-20～100℃、45-95%RH",null,null,null,"北京中科天昊科技有限公司"]
[61,"紫外老化实验机","QUV-SPRAY","20-10602-92-SPRAY",{"$nulls":4},"Q-Lab Corporation"]
[62,"紫外光耐气候试验箱","ZN-P",20110664,"300-700nm；10-80℃",null,"±3℃",null,"无锡苏南试验设备有限公司"]
[63,"超声波探伤仪","EP650-BX-CCC-K",201107607,{"$nulls":4},"奥林巴斯（北京）销售服务有限公司"]
[64,"涡流探伤仪","N600D-CCC",200090509,{"$nulls":4},"奥林巴斯（北京）销售服务有限公司"]
[65,"X射线衍射仪","XRD-6100","Q30345801090",{"$nulls":4},"株式会社岛津制作所"]
[66,"X射线残余应力分析仪","iXRD Combo",20173081020,{"$nulls":4},"Proto Manufacturing"]
[67,"三坐标测量仪","CMM CONTURA 7/10/6",226964,"700×1000×600mm",null,null,"0.1μm","Carl Zeiss IMT(shanghai)Co.,Ltd"]
[68,"恒温恒湿控制仪","MU13","250820210810504",{"$nulls":4},"江苏奥林维尔环境设备有限公司"]
[69,"标准平台","1m*1m",null,"1000×1000mm"]
[70,"小型离子溅射仪","ETD-2000","E-J201001028",{"$nulls":4},"北京博远微纳科技有限公司"]
[71,"热场发射扫描电镜","sigma300",8211011251,"1000000×",null,null,null,"德国蔡司"]
[72,"邵氏硬度计","LX-D",210519027,"100HD",null,null,null,"深圳市时代之峰科技有限公司"]
[73,"智能化导热系数测定仪","DRCD-3030","21-046","10-80℃",null,null,null,"沈阳合兴自动化设备有限公司"]
[74,"热线法导热系数测定仪","KDRX-11",210735,{"$nulls":4},"湘潭湘仪仪器有限公司"]
[75,"低温膨胀仪","PCY-D",210752,"-40～200℃\n±12.7mm",null,null,null,"湘潭湘仪仪器有限公司"]
[76,"热变形维卡软化点温度测定仪","RWCY-E","21-017","室温-200℃",null,null,null,"沈阳合兴自动化设备有限公司"]
[77,"简悬组合冲击试验机","XBL",210920,{"$nulls":4},"济南天辰试验机制造有限公司"]
[78,"高精度导热系数测定仪（平板热流计法）","DRPL-111",210753,{"$nulls":4},"湘潭湘仪仪器有限公司"]
[79,"塑料试样压片机"]
[80,"智能式门窗角强度试验机","JQD-20B",201217,"20kN",null,null,null,"沈阳合兴自动化设备有限公司"]
[81,"智能式门窗力学性能试验机","LXJ2421","21-008",{"$nulls":4},"沈阳合兴自动化设备有限公司"]
[82,"电热恒温水浴锅","SYG-2-4双列四孔",2303334,"室温+5～100℃",null,"±0.5℃",null,"天津市泰斯特仪器有限公司"]
[83,"水紫外线辐照控制仪","SZW-3","2015MFJ004",{"$nulls":4},"郑州惠晟材料科技有限公司河南建材研究设计院"]
[84,"传动锁闭器耐久性试验机","WJ-SBQ","20-01",{"$nulls":4},"沈阳紫薇恒检测设备有限公司"]
[85,"地弹簧寿命试验机","MC-DTH-A","20-01",{"$nulls":4},"沈阳紫薇恒检测设备有限公司"]
[86,"门窗滑轮启闭耐久试验机","WJ-HL-A","20-01",{"$nulls":4},"沈阳紫薇恒检测设备有限公司"]
[87,"插销耐久性试验机","MC-CX-B","21-01",{"$nulls":4},"沈阳紫薇恒检测设备有限公司"]
[88,"门窗防沙尘测试机","MCD","2021-016",{"$nulls":4},"北京中科天昊科技有限公司"]
[89,"直读光谱仪","MAXx LMF15",11003435,{"$nulls":4},"SPECTRO"]
[90,"无级变速迷你型车床","CJ9518D.C3",{"$nulls":5},"上海西马特机械制造有限公司"]
[91,"微机控制电子万能试验机","103A 1KN",1705095,"1KN","0.5级",null,null,"深圳万测试验设备有限公司"]
[92,"电子拉力试验机","LDS-1","036","1000N",null,null,null,"济南思达测试技术有限公司"]
[93,"智能型压缩强度试验机","OT-2",16310,{"$nulls":4},"济南欧拓试验设备有限公司"]
[94,"纸板耐破度测定仪","BLD-608B",2024040301,{"$nulls":4},"东莞博莱德仪器设备有限公司"]
[95,"直流低电阻测试仪","QJ36s",24020619,{"$nulls":4},"上海双特电工仪器有限公司"]
[96,"电子秒表","YS-510","T202108-1",{"$nulls":4},"奕圣"]
[97,"橡胶塑料测厚仪","HD-4型",210913,"0-10mm",null,null,"0.01mm","北京中科路达试验仪器有限公司"]
[98,"A型橡胶硬度计","LD-A","8D17E00259"]
[99,"粘度计","QND-4",40,{"$nulls":4},"天津市精科材料试验机厂"]
[100,"A型硬度计标准块","SHA18008",{"$nulls":5},"泉州市丰泽东海仪器硬度块厂"]
[101,"177ML气动挤胶枪","ZY-Y-JC-170",{"$nulls":5},"沧州中亚试验仪器有限公司"]
[102,"硬度计","LAC-J",42116631]
[103,"涂料涂层耐沾污性试验用灰标准样品",{"$nulls":6},"北京市建筑科学研究院（集团）有限公司研制"]
[104,"涂料涂层耐沾污性试验用灰标准样品",{"$nulls":6},"北京市建筑科学研究院（集团）有限公司研制"]
[105,"旋转粘度计","DVIM",86026984,"100-1000Pa·S",null,null,"0.5Pa·S","奥恒生物Brookfield"]
[106,"精密空调","V23","250820210810504",{"$nulls":4},"江苏奥利维尔环境设备有限公司"]
[107,"电感耦合等离子体发射光谱仪","iCAP 7400 Radial","IC74RC193823","500ppb-100ppm",null,null,null,"ThermoFisher Scientific"]
[108,"电子天平","ATY224","D307510361","220g",null,null,"0.1mg","SHIMADZU"]
[109,"电子天平","JD300-3",134149,"20mg-300g",null,"10mg","1mg","沈阳龙腾电子有限公司"]
[110,"电子天平","BL-220H","D432907040","220g",null,null,"1mg","SHIMADZU Corporation Japan"]
[111,"电子天平","ME55/02","C121841857","1mg-52g","1级","1mg","0.01mg","梅特勒-托利多仪器（上海）有限公司"]
[112,"电子天平","FA20048","400604416855","0.01g-200g","1级","1mg","0.1mg","上海天美天平仪器有限公司"]
[113,"电子天平","DJ-20001","09002","2000g",null,"1g","0.1g","福州华志科学仪器有限公司"]
[114,"数控超声波清洗器","KQ3200DE型",null,"6L",null,null,null,"昆山市超声仪器有限公司"]
[115,"恒温水浴锅","CH-6",342515,"室温+5～100℃",null,null,"0.1℃","江苏金坛宏华仪器厂"]
[116,"实验室级超纯水机","SMART-S2-10DS",2107192605,{"$nulls":4},"南京易普易达科技发展有限公司"]
[117,"微波消解萃取仪","MARS \n6240/50","MJ9431","30-220℃",null,null,null,"CEM"]
[118,"耐溶剂擦拭仪","RJCS",21070521,"999次",null,null,null,"普申检测仪器（上海）有限公司"]
[119,"石墨赶酸器","GSN-24A","GSN24A2200W011"]
[120,"微量水分分析仪","KLS-411","720912N1121030003","10μg-20mg",null,null,"0.01μg","上海仪电科学仪器股份有限公司"]
[121,"电热鼓风干燥箱","101-2DB",2305309,"250℃",null,"±1.0℃",null,"天津市泰斯特仪器有限公司"]
[122,"低温试验箱","DW-40","2021101319040K","-40℃",null,null,null,"沧州华屹试验仪器有限公司"]
[123,"医用低温箱","DW40-120","NO10·3636","-30℃",null,null,null,"沈阳市医疗设备厂"]
[124,"弯折仪","DWZ-120",21101809,{"$nulls":4},"沧州华屹试验仪器有限公司"]
[125,"电热鼓风干燥箱","GZX-9030MBE",12346,"250℃",null,"±1.0℃",null,"上海博迅实业有限公司医疗设备厂"]
[126,"箱式电阻炉","SX2.5-10",2012049,"1000℃",null,null,null,"上海树立仪器仪表有限公司"]
[127,"电热鼓风干燥箱","GZX-9240MBE",3160251,"250℃",null,null,null,"上海博迅实业有限公司医疗设备厂"]
[128,"建筑密封胶相容性试验仪","MW-MX-B","20-11",{"$nulls":4},"沈阳紫薇恒检测设备有限公司"]
[129,"盐雾试验机","Q-FOG/CCT 600","19-34302-51-CCT 600",{"$nulls":4},"Q-Lab Corporation"]
[130,"盐雾试验机","Q-FOG/SSP 600","19-35203-51-SSP600",{"$nulls":4},"Q-Lab Corporation"]
[131,"喷雾腐蚀试验箱","YWF-CASS-750B",2019109,"RT+10～55℃、95-98%RH、1-2ml/80cm2·h",null,null,null,"江苏艾默生试验仪器科技有限公司"]
[132,"二氧化硫腐蚀试验箱","SO2-250",202108146,"RT+10～60℃、≥95%RH、0.05～1%SO2",null,null,null,"南京环科试验设备有限公司"]
[133,"PH计","PHS-3C","600408N0017080420","0-14PH",null,null,0.01,"上海亿电科学仪器股份有限公司"]
[134,"腐蚀试验用划痕器","BGD 1285",12852403036,{"$nulls":4},"标格达精密仪器（广州）有限公司"]
[135,"执手耐久性试验机","MC-ZS-C","20-01",{"$nulls":4},"沈阳紫薇恒检测设备有限公司"]
[136,"合页、滑撑、撑挡耐久性试验机","WJ-HYHC-A","20-01",{"$nulls":4},"沈阳紫薇恒检测设备有限公司"]
[137,"配重"]
[138,"砝码","10kg"]
[139,"耐破强度试验机","OT-3",160311,{"$nulls":4},"济南欧拓试验设备有限公司"]
[140,"影像测量仪","TLS-VMS-2010F","TLS20210716A207","200mm×100mm",null,null,null,"泰勒斯（天津）科技有限公司"]
[141,"自动电位滴定仪","ZDJ-4B","640700N0021010029","10ml\n±1800mV",null,null,"0.001ml\n0.1mV","上海仪电科学仪器股份有限公司"]
[142,"数显恒温油浴锅","HH-S","XR 53667","300℃",null,null,null,"金坛区西城新瑞仪器厂"]
[143,"自动快速卡尔费休水分测定仪","MA-1A","2023032402598674",{"$nulls":4},"上海本昂科学仪器有限公司"]
[144,"秒表","YS-510","T202108-2",{"$nulls":4},"深圳市奕圣科技有限公司"]
[145,"游标卡尺","100cm",23000793,"100cm",null,null,null,"Mitutoyo"]
[146,"高档放大镜",{"$nulls":6},"上海超红光学公司"]
[147,"数显万能角度尺","0-360°","K21F260261","0-360°",null,null,"5′","上海量具刃具厂有限公司"]
[148,"杠杆千分尺","25-50mm","523-122",{"$nulls":4},"Mitutoyo"]
[149,"游标卡尺","200mm",23078115,{"$nulls":4},"Mitutoyo"]
[150,"游标卡尺","200mm",23036697,{"$nulls":4},"Mitutoyo"]
[151,"比色箱","P60+",405807,"750-3200lux",null,null,null,"深圳市天友利标准光源有限公司"]
[152,"百分表","0-10mm",{"$nulls":4},"0.01mm","威海新威量量具有限公司"]
[153,"建材制品燃烧热值测定装置","JCRZ","21-024",{"$nulls":4},"沈阳合兴检测设备有限公司"]
[154,"差式扫描量热仪","DSC3500","206029608-10","-170℃～650℃",null,null,null,"德国耐驰"]
[155,"扭矩测量仪","20Nm",1194,{"$nulls":4},"济南智星电测设备有限公司"]
[156,"微机定硫仪","KZDL-500型",1712012,{"$nulls":4},"鹤壁市华维科力煤质仪器有限公司"]
[157,"节能马弗炉","HD-XL-500",17121318,"1000℃",null,null,null,"鹤壁市华维科力煤质仪器有限公司"]
[158,"电热鼓风干燥箱","101-2DB",2305310,"室温+10～250℃",null,"±1℃",null,"天津市泰斯特仪器有限公司"]
[159,"快速灰分测定仪","KH-3型",{"$nulls":5},"鹤壁市民生科技开发有限责任公司"]
[160,"微机全自动量热仪","ZDHW-5000",201712039,{"$nulls":4},"鹤壁市华维科力煤质仪器有限公司"]
[161,"密封式环保制样粉碎机","GJ-1","HWM21120623",{"$nulls":4},"鹤壁市华维科力煤质仪器有限公司"]
[162,"密封式化验制样粉碎机","GJ-1",6113,{"$nulls":4},"上海光地仪器设备有限公司"]
[163,"建筑材料可燃性试验炉","JL-JCK-3","HY2402402-3259",{"$nulls":4},"河北星蓝建筑仪器有限公司"]
[164,"垂直水平燃烧试验机","ASR-4326",20221229007,{"$nulls":4},"广东艾瑞斯仪器科技有限公司"]
[165,"粉末流动性测试仪","QT-361A",{"$nulls":5},"东莞市启天仪器有限公司"]
[166,"DQ-I电桥专用夹具",null,"0005",{"$nulls":4},"上海双特电工仪器有限公司"]
[167,"空压机","SLPJ-75B","ZA1073",{"$nulls":4},"杭州阿耐斯特岩田友佳空压机有限公司"]
[168,"EDI水处理处理设备","E-0.25T",21051202,{"$nulls":4},"广州顺德济达饮水设备有限公司"]
[169,"反渗透水处理设备","GD-RO-0.5T",21051201,{"$nulls":4},"广州顺德济达饮水设备有限公司"]
[170,"数显显微维氏硬度计","ZHV 30S",206092,"HV0.2-30",null,null,"0.1HV","Zwick/Roell"]
[171,"韦氏硬度计","BSC-W",809234,"20HW",null,null,null,"四合科技"]
[172,"金相显微镜","Lab.A1",3143060142,"100×",null,null,null,"ZEISS"]
[173,"三目体视显微镜","SMZ745",705074,"50×",null,null,null,"Nikon Corporation"]
[174,"电子布氏硬度计","DHB-3000","02863","8-650HBW",null,null,null,"莱州市蔚仪试验器械制造有限公司"]
[175,"读数显微镜",null,20211129]
[176,"标准硬度块","102HBW10/1000","B2105137",{"$nulls":4},"泉州市丰泽东海仪器硬度块厂"]
[177,"标准硬度块","212HBW10/3000","B2104980",{"$nulls":4},"泉州市丰泽东海仪器硬度块厂"]
[178,"洛氏硬度计","HR-150A",2215,{"$nulls":4},"莱州华银试验仪器有限公司"]
[179,"电热鼓风干燥箱","101-2DB",2305290,"室温+10～250℃",null,"±1.0℃",null,"天津市泰斯特仪器有限公司"]
[180,"杯突试验仪","QBJ",201109,{"$nulls":4},"普申检测仪器（上海）有限公司"]
[181,"10倍放大镜","45×22mm","201230379384.4",{"$nulls":4},"浙江博宇光学有限公司"]
[182,"漆膜圆柱弯曲试验器","QTY-32",34,{"$nulls":4},"天津永利达材料试验机有限公司"]
[183,"漆膜冲击器","QCJ-120A型",1051,{"$nulls":4},"天津市世博伟业化玻仪器有限公司"]
[184,"漆膜冲击试验器","QCJ-120型",{"$nulls":5},"天津永利达材料试验机有限公司"]
[185,"涂层耐沾污性冲洗装置","NZW型",181204,"0.01秒-99小时59分",null,null,null,"上海普申化工机械有限公司"]
[186,"智能型反射率仪","SMN-R","C18723","0-100%",null,null,0.001,"深圳速德瑞科技有限公司"]
[187,"漆膜电动附着力试验仪","QFD-型",{"$nulls":5},"天津永利达实验室设备有限公司"]
[188,"橡胶老化试验箱","RLH-250",202108147,"RT+10～300℃",null,null,null,"南京环科试验设备有限公司"]
[189,"湿热试验箱","ETE-HJS-2252","120713-1","RT+10～100℃、90-98%RH",null,null,null,"无锡精创科技有限公司"]
[190,"高低温湿热试验箱","GDJS-100E",202108144,"-70～150℃、20-98%RH",null,null,null,"南京环科试验设备有限公司"]
[191,"周期浸润腐蚀试验箱","ZY-YF-C1",2021092201,{"$nulls":4},"淮安市中亚试验设备有限公司"]
[192,"热循环试验箱","ETE-GDJS-150L","120713-2","-30～100℃",null,null,null,"无锡精创科技有限公司"]
[193,"磨耗仪","JM-IV型",{"$nulls":5},"天津永利达材料试验机有限公司"]
[194,"电子天平","YP30000","YRV07202108002","30000g",null,null,"1g","上海佑科仪器仪表有限公司"]
[195,"金相镶嵌机","XQ-2B",2355,"φ30×15",null,null,null,"莱州市蔚仪试验器械制造有限公司"]
[196,"自动研磨/抛光机","MoPao2S","08055",{"$nulls":4},"莱州市蔚仪试验器械制造有限公司"]
[197,"自动镶嵌机","ZXQ-2",9057,{"$nulls":4},"莱州市蔚仪试验器械制造有限公司"]
[198,"涂层落砂耐磨试验机","ML",{"$nulls":5},"上海乐傲实验仪器有限公司"]
[199,"涂层落砂耐磨试验机","QML-A型",{"$nulls":5},"天津市建仪试验机有限责任公司"]
[200,"手动金相试样切割机","iqiege-160Z","08028",{"$nulls":4},"莱州市蔚仪试验器械制造有限公司"]
[201,"耐压测试仪","JK2673A型","B259",{"$nulls":4},"常州市金科安联科技有限公司"]
[202,"耐辐照试验机","SGR-3",20230104003,"RT+10～60℃",null,null,null,"北京中科天昊科技有限公司"]
[203,"耐紫外光辐照试验箱","ZE-2",20230104002,"50±3℃",null,null,null,"北京中科天昊科技有限公司"]
[204,"霰弹冲击试验仪"]
[205,"中空玻璃露点仪","ZBL-LD-B","21-033","-60～-40℃",null,null,null,"沈阳合兴自动化设备有限公司"]
[206,"表面应力仪","SSM-Ⅱ",606,{"$nulls":4},"中国建筑材料科学研究总院"]
[207,"傅立叶变换红外光谱仪","FTIR920",{"$nulls":5},"北京中科天昊科技有限公司"]
[208,"可见光透射比、遮阳系数测试系统","HX-BRT3600","SST210608H","190-3600nm",null,null,null,"沈阳合兴自动化设备有限公司"]
[209,"惰性气体分析仪","HELOX4","HA-321063",{"$nulls":4},"Helantec GmbH"]
[210,"安全玻璃透射比测定仪","SGT-3","04690121",{"$nulls":4},"北京奥博泰科技有限公司"]
[211,"电子数显卡尺","0-150mm",180826366]
[212,"卡尺","200mm",23039801,{"$nulls":4},"Mitutoyo"]
[213,"辐射率仪"]
[214,"激光电子经纬仪","DT-02","T342399",{"$nulls":4},"南方测绘"]
[215,"数显千分表","543-790"]
[216,"塞尺","0.02-1.00mm"]
[217,"压缩永久变形器","B型","    21-1092",{"$nulls":4},"扬州市道纯试验机械厂"]
[218,"酸缸","10L"]
[219,"酸缸","60L"]
[220,"酸缸","30L"]
[221,"便携式电导率仪","DDBJ-350F","6111700N0021030003","0.1-1*10^4us/cm",null,null,null,"上海仪电科学仪器股份有限公司"]
[222,"变形抗破裂性试验仪"]
[223,"微机控制电液伺服万能试验机","WAW-600"]
[224,"数字涡流金属电导仪"]
[225,"恒温水浴锅"]
[226,"数显邵氏硬度计"]
[227,"超高频数字交流毫伏表"]
[228,"电子天平"]
[229,"电热恒温板"]
[230,"电子天平"]
[231,"电热鼓风干燥箱"]
[232,"超级恒温水浴锅"]
[233,"绝缘电阻测试仪"]